Legrand / Raritan Xerus™ JSON-RPC API for Remote Access Devices like KX4-101, KX3G2

Loading...
Searching...
No Matches
Public Attributes | List of all members
radm::KvmDevice::TemperatureReading Struct Reference

Device temperature reading. More...

`import "KvmDevice.idl";`

## Public Attributes
boolean | available
| Whether the reading data is valid.
float | currentValue
| Current device temperature (in degree Celsius)
float | maximumValue
| Historical temperature maximum (in degree Celsius)
float | minimumValue
| Historical temperature minimum (in degree Celsius)

## Detailed Description

Device temperature reading.

Definition at line 53 of file KvmDevice.idl.

## Member Data Documentation

## ◆ available

boolean radm::KvmDevice::TemperatureReading::available

Whether the reading data is valid.

Definition at line 54 of file KvmDevice.idl.

## ◆ currentValue

float radm::KvmDevice::TemperatureReading::currentValue

Current device temperature (in degree Celsius)

Definition at line 55 of file KvmDevice.idl.

## ◆ maximumValue

float radm::KvmDevice::TemperatureReading::maximumValue

Historical temperature maximum (in degree Celsius)

Definition at line 56 of file KvmDevice.idl.

## ◆ minimumValue

float radm::KvmDevice::TemperatureReading::minimumValue

Historical temperature minimum (in degree Celsius)

Definition at line 57 of file KvmDevice.idl.

The documentation for this struct was generated from the following file:

- KvmDevice.idl