Legrand / Raritan Xerus™ JSON-RPC API for Remote Access Devices like KX4-101, KX3G2

Loading...
Searching...
No Matches
Public Attributes | List of all members
radm::KvmPort::DigitalPortSettings Struct Reference

Settings for digital (non-CIM) ports. More...

`import "KvmPort.idl";`

## Public Attributes
int | edidCycleTime
| Cycle time for hot-plug detect signal on EDID changes (in ms, available for ddc capability)
boolean | vgaMode
| Whether to treat the the video input as originating from an analog video source - if enabled, noise filters and color range conversion are used.
int | vgaGainBoost
| How aggressively color range conversion should be done in VGA mode on a 0..9 scale.
boolean | audioCompensation
| Whether to compensate for issues in HDMI audio connection.

## Detailed Description

Settings for digital (non-CIM) ports.

Definition at line 84 of file KvmPort.idl.

## Member Data Documentation

## ◆ audioCompensation

boolean radm::KvmPort::DigitalPortSettings::audioCompensation

Whether to compensate for issues in HDMI audio connection.

Definition at line 89 of file KvmPort.idl.

## ◆ edidCycleTime

int radm::KvmPort::DigitalPortSettings::edidCycleTime

Cycle time for hot-plug detect signal on EDID changes (in ms, available for ddc capability)

Definition at line 85 of file KvmPort.idl.

## ◆ vgaGainBoost

int radm::KvmPort::DigitalPortSettings::vgaGainBoost

How aggressively color range conversion should be done in VGA mode on a 0..9 scale.

Definition at line 88 of file KvmPort.idl.

## ◆ vgaMode

boolean radm::KvmPort::DigitalPortSettings::vgaMode

Whether to treat the the video input as originating from an analog video source - if enabled, noise filters and color range conversion are used.

Definition at line 86 of file KvmPort.idl.

The documentation for this struct was generated from the following file:

- KvmPort.idl