Legrand / Raritan / Server Technology Xerus™ JSON-RPC API

Loading...
Searching...
No Matches
NumericSensor.idl
1/* SPDX-License-Identifier: BSD-3-Clause */
2/*
3 * Copyright 2009 Raritan Inc. All rights reserved.
4 */
5
6#ifndef __SENSORMODEL_NUMERICSENSOR_IDL__
7#define __SENSORMODEL_NUMERICSENSOR_IDL__
8
9#include <Event.idl>
10#include <Sensor.idl>
11#include <UserEvent.idl>
12
13/** Sensors Model */
14module sensors {
15
16 /** A sensor with numeric readings */
17 interface NumericSensor extends Sensor {
18
19 constant int THRESHOLD_OUT_OF_RANGE = 1; ///< The threshold exceedes the sensor range
20 constant int THRESHOLD_INVALID = 2; ///< The threshold constraints are not met
21 constant int THRESHOLD_NOT_SUPPORTED = 3; ///< The sensor does not support setting this threshold
22
23 /** Range of possible sensor readings */
24 structure Range {
25 double lower; ///< Minimum reading
26 double upper; ///< Maximum reading
27 };
28
29 /**
30 * Threshold capabilities
31 */
32 structure ThresholdCapabilities {
33 boolean hasUpperCritical; ///< Sensor has upper critical threshold
34 boolean hasUpperWarning; ///< Sensor has upper warning threshold
35 boolean hasLowerWarning; ///< Sensor has lower warning threshold
36 boolean hasLowerCritical; ///< Sensor has lower critical threshold
37 };
38
39 /** Numeric sensor metadata */
40 structure MetaData {
41 /**
42 * Sensor type, reading type and unit
43 */
44 Sensor.TypeSpec type;
45
46 /**
47 * Number of significant decimal digits.
48 *
49 * Indicates how many digits should be displayed
50 * to the right of the decimal point. I.e. double
51 * values must be rounded with this precision.
52 */
53 int decdigits;
54
55 /**
56 * Sensor accuracy in percent.
57 *
58 * How close in percent measurement is to actual value.
59 * This value has an implicit precision of 2, i.e. the double
60 * value must be rounded for 2 decimal digits before use.
61 * For example a reading of 10.0 and an accuracy of 0.2
62 * means the actual reading value is 10.0 +/- 0.2%.
63 *
64 * A value of 0 means unused.
65 */
66 float accuracy;
67
68 /**
69 * Sensor resolution.
70 *
71 * Minimum difference between any two measured values.
72 * Must be rounded with decimal digits.
73 */
74 float resolution;
75
76 /**
77 * Sensor tolerance.
78 *
79 * Tolerance is given in +/- counts of the reading value.
80 * It indicates a constant magnitude possible error in the
81 * quantization of an analog input to the sensor.
82 * Rounded with decimal digits + 1.
83 *
84 * A value of 0 means unused.
85 */
86 float tolerance;
87
88 /**
89 * Sensor noise threshold.
90 *
91 * Threshold under which sensor measurements will be ignored.
92 * Sensor measurements below that value will be reported at
93 * the lower bound of the sensor range.
94 */
95 float noiseThreshold;
96
97 /**
98 * Range of possible sensor readings.
99 *
100 * Range values are rounded with with decimal digits.
101 */
102 Range range;
103
104 /**
105 * Threshold capabilities
106 */
107 ThresholdCapabilities thresholdCaps;
108 };
109
110 /** Numeric sensor thresholds */
111 structure Thresholds {
112 boolean upperCriticalActive; ///< \c true if the upper critical threshold is enabled
113 double upperCritical; ///< Upper critical threshold
114 boolean upperWarningActive; ///< \c true if the upper warning threshold is enabled
115 double upperWarning; ///< Upper warning threshold
116 boolean lowerWarningActive; ///< \c true if the lower warning threshold is enabled
117 double lowerWarning; ///< Lower warning threshold
118 boolean lowerCriticalActive; ///< \c true if the lower critical threshold is enabled
119 double lowerCritical; ///< Lower critical threshold
120 int assertionTimeout; ///< Assertion timeout in samples
121 float deassertionHysteresis; ///< Deassertion hysteresis
122 };
123
124 /** Numeric sensor reading */
125 structure Reading {
126 /** Numeric sensor status
127 *
128 * The status is determined on the basis of rounded values. The
129 * rounding is done according to MetaData::decdigits. This ensures
130 * that status and value will match when displayed simultaneously,
131 * if the value is also displayed rounded.
132 */
133 structure Status {
134 boolean aboveUpperCritical; ///< Reading is above upper critical threshold
135 boolean aboveUpperWarning; ///< Reading is above upper warning threshold
136 boolean belowLowerWarning; ///< Reading is below lower warning threshold
137 boolean belowLowerCritical; ///< Reading is below lower critical threshold
138 };
139 time timestamp; ///< UNIX timestamp (UTC) of last sample
140 boolean available; ///< \c true if the sensor is available
141 Status status; ///< Numeric sensor status
142 boolean valid; ///< \c true if the sensor reading is valid
143 double value; ///< Numeric sensor reading, not rounded
144 };
145
146 /** Numeric sensor minimum / maximum values */
147 structure MinMax {
148 double minReading; ///< the minimum value since observedSince, not rounded
149 time minReadingTimestamp; ///< UNIX timestamp (UTC) when the minimum value has occurred
150 double maxReading; ///< the maximum value since observedSince, not rounded
151 time maxReadingTimestamp; ///< UNIX timestamp (UTC) when the maximum value has occurred
152 boolean valid; ///< \c true if min and max are valid
153 time observedSince; ///< UNIX timestamp (UTC) of last reset of min / max
154 };
155
156 /** Event: Numeric sensor reading has changed
157 *
158 * The event is sent when the Reading::value has changed enough to affect
159 * a digit to be displayed according to MetaData::decdigits, or if one of
160 * Reading::available, Reading::status or Reading::valid has changed.
161 */
162 valueobject ReadingChangedEvent extends idl.Event {
163 Reading newReading; ///< New numeric sensor reading
164 };
165
166 /** Event: Sensor state has changed */
167 valueobject StateChangedEvent extends idl.Event {
168 Reading oldReading; ///< Reading before state change
169 Reading newReading; ///< Reading after state change
170 };
171
172 /** Event: Sensor metadata has changed */
173 valueobject MetaDataChangedEvent extends idl.Event {
174 MetaData oldMetaData; ///< Metadata before change
175 MetaData newMetaData; ///< Metadata after change
176 };
177
178 /** Event: Sensor default thresholds have changed */
179 valueobject DefaultThresholdsChangedEvent extends event.UserEvent {
180 Thresholds oldDefaultThresholds; ///< Default thresholds set before change
181 Thresholds newDefaultThresholds; ///< Default thresholds set after change
182 };
183
184 /** Event: Sensor thresholds have changed */
185 valueobject ThresholdsChangedEvent extends event.UserEvent {
186 Thresholds oldThresholds; ///< Threshold set before change
187 Thresholds newThresholds; ///< Threshold set after change
188 };
189
190 /** Event: Sensor min or max value has changed
191 *
192 * The event is sent when MinMax::minReading or MinMax::maxReading have
193 * changed enough to affect a digit to be displayed according to MetaData::decdigits,
194 * or if MinMax::valid has changed.
195 */
196 valueobject MinMaxChangedEvent extends idl.Event {
197 MinMax newMinMax; ///< Minimum / maximum of sensor value
198 };
199
200 /** Event: Min / Max value has been reset */
201 valueobject MinMaxResetEvent extends event.UserEvent {
202 MinMax oldMinMax; ///< Min / max before reset
203 MinMax newMinMax; ///< Min / max after reset, incl. new observedSince timestamp
204 };
205
206 /**
207 * Retrieve the sensor metadata.
208 *
209 * @return Sensor metadata
210 */
211 MetaData getMetaData();
212
213 /**
214 * Retrieve the sensor default thresholds.
215 *
216 * @return Set of default thresholds
217 */
218 Thresholds getDefaultThresholds();
219
220 /**
221 * Retrieve the thresholds.
222 *
223 * Note: In case of peripheral devices these thresholds may be overridden
224 * by the device slot configuration.
225 *
226 * @return Set of configured thresholds
227 */
228 Thresholds getThresholds();
229
230 /**
231 * Change the thresholds.
232 *
233 * Note: In case of peripheral devices these thresholds may be overridden
234 * by the device slot configuration.
235 *
236 * @param thresh New set of thresholds
237 *
238 * @return 0 if OK
239 * @return THRESHOLD_OUT_OF_RANGE if any threshold is out of range
240 * @return THRESHOLD_INVALID if thresholds don't meet the requirements
241 * @return THRESHOLD_NOT_SUPPORTED if threshold is not supported
242 */
243 int setThresholds(in Thresholds thresh);
244
245 /**
246 * Get the sensor reading.
247 *
248 * @return Sensor reading, not rounded
249 */
250 Reading getReading();
251
252 /**
253 * Get the min / max of sensor value.
254 *
255 * @return Sensor min / max values
256 */
257 MinMax getMinMax();
258
259 /**
260 * Reset min / max of sensor value.
261 *
262 */
263 void resetMinMax();
264
265 };
266
267}
268
269#endif
sensors::NumericSensor
A sensor with numeric readings.
Definition NumericSensor.idl:17
sensors::NumericSensor::resetMinMax
void resetMinMax()
Reset min / max of sensor value.
sensors::NumericSensor::THRESHOLD_INVALID
constant int THRESHOLD_INVALID
The threshold constraints are not met.
Definition NumericSensor.idl:20
sensors::NumericSensor::getReading
Reading getReading()
Get the sensor reading.
sensors::NumericSensor::getThresholds
Thresholds getThresholds()
Retrieve the thresholds.
sensors::NumericSensor::getDefaultThresholds
Thresholds getDefaultThresholds()
Retrieve the sensor default thresholds.
sensors::NumericSensor::getMinMax
MinMax getMinMax()
Get the min / max of sensor value.
sensors::NumericSensor::THRESHOLD_NOT_SUPPORTED
constant int THRESHOLD_NOT_SUPPORTED
The sensor does not support setting this threshold.
Definition NumericSensor.idl:21
sensors::NumericSensor::getMetaData
MetaData getMetaData()
Retrieve the sensor metadata.
sensors::NumericSensor::setThresholds
int setThresholds(in Thresholds thresh)
Change the thresholds.
sensors::NumericSensor::THRESHOLD_OUT_OF_RANGE
constant int THRESHOLD_OUT_OF_RANGE
The threshold exceedes the sensor range.
Definition NumericSensor.idl:19
sensors::Sensor
Sensor interface
Definition Sensor.idl:15
idl
Basic IDL definitions.
Definition Event.idl:10
sensors
Sensors Model.
Definition AccumulatingNumericSensor.idl:13
idl::Event
Common base for all events.
Definition Event.idl:13
sensors::NumericSensor::DefaultThresholdsChangedEvent
Event: Sensor default thresholds have changed.
Definition NumericSensor.idl:179
sensors::NumericSensor::DefaultThresholdsChangedEvent::oldDefaultThresholds
Thresholds oldDefaultThresholds
Default thresholds set before change.
Definition NumericSensor.idl:180
sensors::NumericSensor::DefaultThresholdsChangedEvent::newDefaultThresholds
Thresholds newDefaultThresholds
Default thresholds set after change.
Definition NumericSensor.idl:181
sensors::NumericSensor::MetaDataChangedEvent
Event: Sensor metadata has changed.
Definition NumericSensor.idl:173
sensors::NumericSensor::MetaDataChangedEvent::oldMetaData
MetaData oldMetaData
Metadata before change.
Definition NumericSensor.idl:174
sensors::NumericSensor::MetaDataChangedEvent::newMetaData
MetaData newMetaData
Metadata after change.
Definition NumericSensor.idl:175
sensors::NumericSensor::MetaData
Numeric sensor metadata.
Definition NumericSensor.idl:40
sensors::NumericSensor::MetaData::type
Sensor::TypeSpec type
Sensor type, reading type and unit.
Definition NumericSensor.idl:44
sensors::NumericSensor::MetaData::resolution
float resolution
Sensor resolution.
Definition NumericSensor.idl:74
sensors::NumericSensor::MetaData::noiseThreshold
float noiseThreshold
Sensor noise threshold.
Definition NumericSensor.idl:95
sensors::NumericSensor::MetaData::tolerance
float tolerance
Sensor tolerance.
Definition NumericSensor.idl:86
sensors::NumericSensor::MetaData::accuracy
float accuracy
Sensor accuracy in percent.
Definition NumericSensor.idl:66
sensors::NumericSensor::MetaData::range
Range range
Range of possible sensor readings.
Definition NumericSensor.idl:102
sensors::NumericSensor::MetaData::decdigits
int decdigits
Number of significant decimal digits.
Definition NumericSensor.idl:53
sensors::NumericSensor::MetaData::thresholdCaps
ThresholdCapabilities thresholdCaps
Threshold capabilities.
Definition NumericSensor.idl:107
sensors::NumericSensor::MinMaxChangedEvent
Event: Sensor min or max value has changed.
Definition NumericSensor.idl:196
sensors::NumericSensor::MinMaxChangedEvent::newMinMax
MinMax newMinMax
Minimum / maximum of sensor value.
Definition NumericSensor.idl:197
sensors::NumericSensor::MinMaxResetEvent
Event: Min / Max value has been reset.
Definition NumericSensor.idl:201
sensors::NumericSensor::MinMaxResetEvent::oldMinMax
MinMax oldMinMax
Min / max before reset.
Definition NumericSensor.idl:202
sensors::NumericSensor::MinMaxResetEvent::newMinMax
MinMax newMinMax
Min / max after reset, incl. new observedSince timestamp.
Definition NumericSensor.idl:203
sensors::NumericSensor::MinMax
Numeric sensor minimum / maximum values.
Definition NumericSensor.idl:147
sensors::NumericSensor::MinMax::maxReadingTimestamp
time maxReadingTimestamp
UNIX timestamp (UTC) when the maximum value has occurred.
Definition NumericSensor.idl:151
sensors::NumericSensor::MinMax::minReading
double minReading
the minimum value since observedSince, not rounded
Definition NumericSensor.idl:148
sensors::NumericSensor::MinMax::valid
boolean valid
true if min and max are valid
Definition NumericSensor.idl:152
sensors::NumericSensor::MinMax::minReadingTimestamp
time minReadingTimestamp
UNIX timestamp (UTC) when the minimum value has occurred.
Definition NumericSensor.idl:149
sensors::NumericSensor::MinMax::observedSince
time observedSince
UNIX timestamp (UTC) of last reset of min / max.
Definition NumericSensor.idl:153
sensors::NumericSensor::MinMax::maxReading
double maxReading
the maximum value since observedSince, not rounded
Definition NumericSensor.idl:150
sensors::NumericSensor::Range
Range of possible sensor readings.
Definition NumericSensor.idl:24
sensors::NumericSensor::Range::upper
double upper
Maximum reading.
Definition NumericSensor.idl:26
sensors::NumericSensor::Range::lower
double lower
Minimum reading.
Definition NumericSensor.idl:25
sensors::NumericSensor::ReadingChangedEvent
Event: Numeric sensor reading has changed.
Definition NumericSensor.idl:162
sensors::NumericSensor::ReadingChangedEvent::newReading
Reading newReading
New numeric sensor reading.
Definition NumericSensor.idl:163
sensors::NumericSensor::Reading::Status
Numeric sensor status.
Definition NumericSensor.idl:133
sensors::NumericSensor::Reading::Status::aboveUpperCritical
boolean aboveUpperCritical
Reading is above upper critical threshold.
Definition NumericSensor.idl:134
sensors::NumericSensor::Reading::Status::belowLowerWarning
boolean belowLowerWarning
Reading is below lower warning threshold.
Definition NumericSensor.idl:136
sensors::NumericSensor::Reading::Status::belowLowerCritical
boolean belowLowerCritical
Reading is below lower critical threshold.
Definition NumericSensor.idl:137
sensors::NumericSensor::Reading::Status::aboveUpperWarning
boolean aboveUpperWarning
Reading is above upper warning threshold.
Definition NumericSensor.idl:135
sensors::NumericSensor::Reading
Numeric sensor reading.
Definition NumericSensor.idl:125
sensors::NumericSensor::Reading::status
Status status
Numeric sensor status.
Definition NumericSensor.idl:141
sensors::NumericSensor::Reading::available
boolean available
true if the sensor is available
Definition NumericSensor.idl:140
sensors::NumericSensor::Reading::value
double value
Numeric sensor reading, not rounded.
Definition NumericSensor.idl:143
sensors::NumericSensor::Reading::valid
boolean valid
true if the sensor reading is valid
Definition NumericSensor.idl:142
sensors::NumericSensor::Reading::timestamp
time timestamp
UNIX timestamp (UTC) of last sample.
Definition NumericSensor.idl:139
sensors::NumericSensor::StateChangedEvent
Event: Sensor state has changed.
Definition NumericSensor.idl:167
sensors::NumericSensor::StateChangedEvent::oldReading
Reading oldReading
Reading before state change.
Definition NumericSensor.idl:168
sensors::NumericSensor::StateChangedEvent::newReading
Reading newReading
Reading after state change.
Definition NumericSensor.idl:169
sensors::NumericSensor::ThresholdCapabilities
Threshold capabilities.
Definition NumericSensor.idl:32
sensors::NumericSensor::ThresholdCapabilities::hasUpperCritical
boolean hasUpperCritical
Sensor has upper critical threshold.
Definition NumericSensor.idl:33
sensors::NumericSensor::ThresholdCapabilities::hasLowerWarning
boolean hasLowerWarning
Sensor has lower warning threshold.
Definition NumericSensor.idl:35
sensors::NumericSensor::ThresholdCapabilities::hasUpperWarning
boolean hasUpperWarning
Sensor has upper warning threshold.
Definition NumericSensor.idl:34
sensors::NumericSensor::ThresholdCapabilities::hasLowerCritical
boolean hasLowerCritical
Sensor has lower critical threshold.
Definition NumericSensor.idl:36
sensors::NumericSensor::ThresholdsChangedEvent
Event: Sensor thresholds have changed.
Definition NumericSensor.idl:185
sensors::NumericSensor::ThresholdsChangedEvent::newThresholds
Thresholds newThresholds
Threshold set after change.
Definition NumericSensor.idl:187
sensors::NumericSensor::ThresholdsChangedEvent::oldThresholds
Thresholds oldThresholds
Threshold set before change.
Definition NumericSensor.idl:186
sensors::NumericSensor::Thresholds
Numeric sensor thresholds.
Definition NumericSensor.idl:111
sensors::NumericSensor::Thresholds::upperWarningActive
boolean upperWarningActive
true if the upper warning threshold is enabled
Definition NumericSensor.idl:114
sensors::NumericSensor::Thresholds::upperWarning
double upperWarning
Upper warning threshold.
Definition NumericSensor.idl:115
sensors::NumericSensor::Thresholds::assertionTimeout
int assertionTimeout
Assertion timeout in samples.
Definition NumericSensor.idl:120
sensors::NumericSensor::Thresholds::lowerWarningActive
boolean lowerWarningActive
true if the lower warning threshold is enabled
Definition NumericSensor.idl:116
sensors::NumericSensor::Thresholds::upperCritical
double upperCritical
Upper critical threshold.
Definition NumericSensor.idl:113
sensors::NumericSensor::Thresholds::lowerCriticalActive
boolean lowerCriticalActive
true if the lower critical threshold is enabled
Definition NumericSensor.idl:118
sensors::NumericSensor::Thresholds::lowerWarning
double lowerWarning
Lower warning threshold.
Definition NumericSensor.idl:117
sensors::NumericSensor::Thresholds::deassertionHysteresis
float deassertionHysteresis
Deassertion hysteresis.
Definition NumericSensor.idl:121
sensors::NumericSensor::Thresholds::lowerCritical
double lowerCritical
Lower critical threshold.
Definition NumericSensor.idl:119
sensors::NumericSensor::Thresholds::upperCriticalActive
boolean upperCriticalActive
true if the upper critical threshold is enabled
Definition NumericSensor.idl:112
sensors::Sensor::TypeSpec
Complete sensor type specification.
Definition Sensor.idl:177