Legrand / Raritan / Server Technology Xerus™ JSON-RPC API

Loading...
Searching...
No Matches
Classes | Public Member Functions | Public Attributes | List of all members
sensors::Logger Interface Reference

Sensor logger interface. More...

`import "SensorLogger.idl";`

## Classes
struct | Info
| Sensor logger info. More...
struct | InfoChangedEvent
| Event: Sensor logger info has changed. More...
struct | LoggedSensorsChangedEvent
| Event: Set of logged sensors has been changed. More...
struct | LogRow
| One full log row. More...
struct | Record
| Sensor log record. More...
struct | SensorSet
| Set of logged sensors. More...
struct | Settings
| Sensor logger settings. More...
struct | SettingsChangedEvent
| Event: Sensor logger settings have been changed. More...
struct | TimedRecord
| Sensor log record with timestamp. More...

## Public Member Functions
Info | getInfo ()
| Retrieve the sensor logger info.
Settings | getSettings ()
| Retrieve the sensor logger settings.
int | setSettings (in Settings settings)
| Change the sensor logger settings.
int | getTimeStamps (out vector< time > timestamps, in int recid, in int count)
| Retrieve a set of log record timestamps.
int | getSensorRecords (out vector< Record > recs, in sensors::Sensor sensor, in int recid, in int count)
| Retrieve log records for a given sensor.
int | getPeripheralDeviceRecords (out vector< Record > recs, in peripheral::DeviceSlot slot, in int recid, in int count)
| Retrieve log records for an peripheral device slot.
int | getSensorTimedRecords (out vector< TimedRecord > recs, in sensors::Sensor sensor, in int recid, in int count)
| Retrieve log records with timestamps for a given sensor.
int | getPeripheralDeviceTimedRecords (out vector< TimedRecord > recs, in peripheral::DeviceSlot slot, in int recid, in int count)
| Retrieve log records with timestamps for an peripheral device slot.
SensorSet | getLoggedSensors ()
| Retrieve the set of logged sensors.
int | setLoggedSensors (in SensorSet sensors)
| Change the set of logged sensors.
int | enableSensors (in SensorSet sensors)
| Enable logging for one or more sensors or peripheral device slots.
int | disableSensors (in SensorSet sensors)
| Disable logging for one or more sensors or peripheral device slots.
boolean | isSensorEnabled (in sensors::Sensor sensor)
| Check if logging is enabled for a given sensor.
boolean | isSlotEnabled (in peripheral::DeviceSlot slot)
| Check if logging is enabled for a given peripheral device slot.
void | enableAllSensors ()
| Enable logging for all PDU sensors.
void | disableAllSensors ()
| Disable logging for all PDU sensors.
time | getSensorSetTimestamp ()
| Get the time of the last sensor set modification.
int | getLogRow (out LogRow row, in int recid)
| Get one full log row.

## Public Attributes
constant int | STATE_UNAVAILABLE = 0
| Sensor state in log record.
constant int | STATE_OPEN = 1
| Circuit breaker open.
constant int | STATE_CLOSE = 2
| Circuit breaker closed.
constant int | STATE_BELOW_LOWER_CRITICAL = 3
| Numeric sensor below lower critical threshold.
constant int | STATE_BELOW_LOWER_WARNING = 4
| Numeric sensor below lower warning threshold.
constant int | STATE_NORMAL = 5
| Numeric sensor in normal range; normal operation.
constant int | STATE_ABOVE_UPPER_WARNING = 6
| Numeric sensor above upper warning threshold.
constant int | STATE_ABOVE_UPPER_CRITICAL = 7
| Numeric sensor above upper critical threshold.
constant int | STATE_ON = 8
| Power state on.
constant int | STATE_OFF = 9
| Power state off.
constant int | STATE_ALARMED = 10
| Alarmed.
constant int | STATE_OK = 11
| OK.
constant int | STATE_MARGINAL = 12
| Marginal.
constant int | STATE_FAIL = 13
| Fail.
constant int | STATE_YES = 14
| Yes.
constant int | STATE_NO = 15
| No.
constant int | STATE_STANDBY = 16
| Standby operation.
constant int | STATE_ONE = 17
| First source active.
constant int | STATE_TWO = 18
| Second source active.
constant int | STATE_IN_SYNC = 19
| Phases are in sync.
constant int | STATE_OUT_OF_SYNC = 20
| Phases are out of sync.
constant int | STATE_FAULT = 21
| Fault.
constant int | STATE_SELF_TEST = 22
| Sensor is currently testing itself.
constant int | STATE_I1_OPEN_FAULT = 23
| Inlet 1 switch open fault.
constant int | STATE_I1_SHORT_FAULT = 24
| Inlet 1 switch short fault.
constant int | STATE_I2_OPEN_FAULT = 25
| Inlet 2 switch open fault.
constant int | STATE_I2_SHORT_FAULT = 26
| Inlet 2 switch short fault.
constant int | STATE_WARNING = 27
| Warning.
constant int | STATE_CRITICAL = 28
| Critical.
constant int | STATE_NON_REDUNDANT = 29
| Non-redundant operation.
constant int | STATE_INACTIVE = 30
| Bypass inactive.
constant int | STATE_BYPASS_SELECTED_BUT_INACTIVE = 31
| Bypass selected but inactive.
constant int | STATE_I1_ACTIVE = 32
| Inlet 1 active.
constant int | STATE_I2_ACTIVE = 33
| Inlet 2 active.
constant int | STATE_BYPASS_ACTIVE = 34
| Operational state: bypass active.

## Detailed Description

Sensor logger interface.

The sensor log stores a fixed number of log records for each enabled sensor. Log records hold the minimum, maximum and average reading of all samples within the period as well as the most critical state.

Record IDs start at 1 and grow continuously without wrap-around. To avoid race conditions it is allowed to request records that are no longer available, i.e. have rotated out of the log. Unavailable records come back empty (available = false, timestamp = 0). It is not OK to read past newestRecId.

Log record periods are synchronized with the system time, so all devices with the same log settings and proper time configuration move to a new record simultaneously.

Definition at line 31 of file SensorLogger.idl.

## Member Function Documentation

## ◆ disableSensors()

int sensors::Logger::disableSensors | ( | in SensorSet | sensors | ) |

Disable logging for one or more sensors or peripheral device slots.

Sensors in the list that are not logged are ignored. Logged sensors not in the list remain enabled.

Parameters

  sensors | Sensors and slots to be disabled

Returns
  0 if OK
  1 if any sensor in the list is unknown

## ◆ enableSensors()

int sensors::Logger::enableSensors | ( | in SensorSet | sensors | ) |

Enable logging for one or more sensors or peripheral device slots.

Sensors in the list that are already logged are ignored. Logged sensors not in the list remain enabled.

Parameters

  sensors | Sensors and slots to be logged

Returns
  0 if OK
  1 if any sensor in the list is unknown

## ◆ getInfo()

Info sensors::Logger::getInfo | ( |  | ) |

Retrieve the sensor logger info.

Returns
  Sensor logger info

## ◆ getLoggedSensors()

SensorSet sensors::Logger::getLoggedSensors | ( |  | ) |

Retrieve the set of logged sensors.

Returns
  Set of logged sensors

## ◆ getLogRow()

int sensors::Logger::getLogRow | ( | out LogRow | row,
|  | in int | recid )

Get one full log row.

Parameters

  row | Result: Log row
  recid | Record id

Returns
  0 if OK
  1 if the record id is invalid

## ◆ getPeripheralDeviceRecords()

int sensors::Logger::getPeripheralDeviceRecords | ( | out vector< Record > | recs,
|  | in peripheral::DeviceSlot | slot,
|  | in int | recid,
|  | in int | count )

Retrieve log records for an peripheral device slot.

Parameters

  recs | Result: Sensor log records
  slot | Peripheral device slot reference
  recid | First record id
  count | Number of records

Returns
  0 if OK
  1 if any record id is invalid

## ◆ getPeripheralDeviceTimedRecords()

int sensors::Logger::getPeripheralDeviceTimedRecords | ( | out vector< TimedRecord > | recs,
|  | in peripheral::DeviceSlot | slot,
|  | in int | recid,
|  | in int | count )

Retrieve log records with timestamps for an peripheral device slot.

Parameters

  recs | Result: Sensor log records
  slot | Peripheral device slot reference
  recid | First record id
  count | Number of records

Returns
  0 if OK
  1 if any record id is invalid

## ◆ getSensorRecords()

int sensors::Logger::getSensorRecords | ( | out vector< Record > | recs,
|  | in sensors::Sensor | sensor,
|  | in int | recid,
|  | in int | count )

Retrieve log records for a given sensor.

Parameters

  recs | Result: Sensor log records
  sensor | Sensor reference
  recid | First record id
  count | Number of records

Returns
  0 if OK
  1 if any record id is invalid

## ◆ getSensorSetTimestamp()

time sensors::Logger::getSensorSetTimestamp | ( |  | ) |

Get the time of the last sensor set modification.

This can be used by clients which keep a cached copy of the sensor set to determine whether that copy is still up-to-date.

Returns
  Sensor set time stamp (UNIX timestamp, UTC)

## ◆ getSensorTimedRecords()

int sensors::Logger::getSensorTimedRecords | ( | out vector< TimedRecord > | recs,
|  | in sensors::Sensor | sensor,
|  | in int | recid,
|  | in int | count )

Retrieve log records with timestamps for a given sensor.

Parameters

  recs | Result: Sensor log records
  sensor | Sensor reference
  recid | First record id
  count | Number of records

Returns
  0 if OK
  1 if any record id is invalid

## ◆ getSettings()

Settings sensors::Logger::getSettings | ( |  | ) |

Retrieve the sensor logger settings.

Returns
  Sensor logger settings

## ◆ getTimeStamps()

int sensors::Logger::getTimeStamps | ( | out vector< time > | timestamps,
|  | in int | recid,
|  | in int | count )

Retrieve a set of log record timestamps.

Parameters

  timestamps | Result: Log record timestamps
  recid | First record id
  count | Number of records

Returns
  0 if OK
  1 if any record id is invalid

## ◆ isSensorEnabled()

boolean sensors::Logger::isSensorEnabled | ( | in sensors::Sensor | sensor | ) |

Check if logging is enabled for a given sensor.

Parameters

  sensor | Sensor to be checked

Returns
  `true` if sensor is logged, `false` otherwise

## ◆ isSlotEnabled()

boolean sensors::Logger::isSlotEnabled | ( | in peripheral::DeviceSlot | slot | ) |

Check if logging is enabled for a given peripheral device slot.

Parameters

  sensor | Peripheral device slot to be checked

Returns
  `true` if slot is logged, `false` otherwise

## ◆ setLoggedSensors()

int sensors::Logger::setLoggedSensors | ( | in SensorSet | sensors | ) |

Change the set of logged sensors.

Parameters

  sensors | New set of sensors

Returns
  0 if OK
  1 if any sensor in the list is unknown

## ◆ setSettings()

int sensors::Logger::setSettings | ( | in Settings | settings | ) |

Change the sensor logger settings.

Parameters

  settings | New settings

Returns
  0 if OK
  1 if any parameters are invalid

## Member Data Documentation

## ◆ STATE_ABOVE_UPPER_CRITICAL

constant int sensors::Logger::STATE_ABOVE_UPPER_CRITICAL = 7

Numeric sensor above upper critical threshold.

Definition at line 110 of file SensorLogger.idl.

## ◆ STATE_ABOVE_UPPER_WARNING

constant int sensors::Logger::STATE_ABOVE_UPPER_WARNING = 6

Numeric sensor above upper warning threshold.

Definition at line 109 of file SensorLogger.idl.

## ◆ STATE_ALARMED

constant int sensors::Logger::STATE_ALARMED = 10

Alarmed.

Definition at line 113 of file SensorLogger.idl.

## ◆ STATE_BELOW_LOWER_CRITICAL

constant int sensors::Logger::STATE_BELOW_LOWER_CRITICAL = 3

Numeric sensor below lower critical threshold.

Definition at line 106 of file SensorLogger.idl.

## ◆ STATE_BELOW_LOWER_WARNING

constant int sensors::Logger::STATE_BELOW_LOWER_WARNING = 4

Numeric sensor below lower warning threshold.

Definition at line 107 of file SensorLogger.idl.

## ◆ STATE_BYPASS_ACTIVE

constant int sensors::Logger::STATE_BYPASS_ACTIVE = 34

Operational state: bypass active.

Definition at line 137 of file SensorLogger.idl.

## ◆ STATE_BYPASS_SELECTED_BUT_INACTIVE

constant int sensors::Logger::STATE_BYPASS_SELECTED_BUT_INACTIVE = 31

Bypass selected but inactive.

Definition at line 134 of file SensorLogger.idl.

## ◆ STATE_CLOSE

constant int sensors::Logger::STATE_CLOSE = 2

Circuit breaker closed.

Definition at line 105 of file SensorLogger.idl.

## ◆ STATE_CRITICAL

constant int sensors::Logger::STATE_CRITICAL = 28

Critical.

Definition at line 131 of file SensorLogger.idl.

## ◆ STATE_FAIL

constant int sensors::Logger::STATE_FAIL = 13

Fail.

Definition at line 116 of file SensorLogger.idl.

## ◆ STATE_FAULT

constant int sensors::Logger::STATE_FAULT = 21

Fault.

Definition at line 124 of file SensorLogger.idl.

## ◆ STATE_I1_ACTIVE

constant int sensors::Logger::STATE_I1_ACTIVE = 32

Inlet 1 active.

Definition at line 135 of file SensorLogger.idl.

## ◆ STATE_I1_OPEN_FAULT

constant int sensors::Logger::STATE_I1_OPEN_FAULT = 23

Inlet 1 switch open fault.

Definition at line 126 of file SensorLogger.idl.

## ◆ STATE_I1_SHORT_FAULT

constant int sensors::Logger::STATE_I1_SHORT_FAULT = 24

Inlet 1 switch short fault.

Definition at line 127 of file SensorLogger.idl.

## ◆ STATE_I2_ACTIVE

constant int sensors::Logger::STATE_I2_ACTIVE = 33

Inlet 2 active.

Definition at line 136 of file SensorLogger.idl.

## ◆ STATE_I2_OPEN_FAULT

constant int sensors::Logger::STATE_I2_OPEN_FAULT = 25

Inlet 2 switch open fault.

Definition at line 128 of file SensorLogger.idl.

## ◆ STATE_I2_SHORT_FAULT

constant int sensors::Logger::STATE_I2_SHORT_FAULT = 26

Inlet 2 switch short fault.

Definition at line 129 of file SensorLogger.idl.

## ◆ STATE_IN_SYNC

constant int sensors::Logger::STATE_IN_SYNC = 19

Phases are in sync.

Definition at line 122 of file SensorLogger.idl.

## ◆ STATE_INACTIVE

constant int sensors::Logger::STATE_INACTIVE = 30

Bypass inactive.

Definition at line 133 of file SensorLogger.idl.

## ◆ STATE_MARGINAL

constant int sensors::Logger::STATE_MARGINAL = 12

Marginal.

Definition at line 115 of file SensorLogger.idl.

## ◆ STATE_NO

constant int sensors::Logger::STATE_NO = 15

No.

Definition at line 118 of file SensorLogger.idl.

## ◆ STATE_NON_REDUNDANT

constant int sensors::Logger::STATE_NON_REDUNDANT = 29

Non-redundant operation.

Definition at line 132 of file SensorLogger.idl.

## ◆ STATE_NORMAL

constant int sensors::Logger::STATE_NORMAL = 5

Numeric sensor in normal range; normal operation.

Definition at line 108 of file SensorLogger.idl.

## ◆ STATE_OFF

constant int sensors::Logger::STATE_OFF = 9

Power state off.

Definition at line 112 of file SensorLogger.idl.

## ◆ STATE_OK

constant int sensors::Logger::STATE_OK = 11

OK.

Definition at line 114 of file SensorLogger.idl.

## ◆ STATE_ON

constant int sensors::Logger::STATE_ON = 8

Power state on.

Definition at line 111 of file SensorLogger.idl.

## ◆ STATE_ONE

constant int sensors::Logger::STATE_ONE = 17

First source active.

Definition at line 120 of file SensorLogger.idl.

## ◆ STATE_OPEN

constant int sensors::Logger::STATE_OPEN = 1

Circuit breaker open.

Definition at line 104 of file SensorLogger.idl.

## ◆ STATE_OUT_OF_SYNC

constant int sensors::Logger::STATE_OUT_OF_SYNC = 20

Phases are out of sync.

Definition at line 123 of file SensorLogger.idl.

## ◆ STATE_SELF_TEST

constant int sensors::Logger::STATE_SELF_TEST = 22

Sensor is currently testing itself.

Definition at line 125 of file SensorLogger.idl.

## ◆ STATE_STANDBY

constant int sensors::Logger::STATE_STANDBY = 16

Standby operation.

Definition at line 119 of file SensorLogger.idl.

## ◆ STATE_TWO

constant int sensors::Logger::STATE_TWO = 18

Second source active.

Definition at line 121 of file SensorLogger.idl.

## ◆ STATE_UNAVAILABLE

constant int sensors::Logger::STATE_UNAVAILABLE = 0

Sensor state in log record.

Unavailable

Definition at line 103 of file SensorLogger.idl.

## ◆ STATE_WARNING

constant int sensors::Logger::STATE_WARNING = 27

Warning.

Definition at line 130 of file SensorLogger.idl.

## ◆ STATE_YES

constant int sensors::Logger::STATE_YES = 14

Yes.

Definition at line 117 of file SensorLogger.idl.

The documentation for this interface was generated from the following file:

- SensorLogger.idl