Legrand / Raritan Xerus™ JSON-RPC API for Remote Access Devices like KX4-101, KX3G2

Loading...
Searching...
No Matches
Public Attributes | List of all members
radm::LocalPort::Settings Struct Reference

Local port settings. More...

`import "LocalPort.idl";`

## Public Attributes
boolean | enabled
| Whether local port UI is enabled or not.
KeyboardLayout | keyboardLayout
| Keyboard language to use.
HotKey | hotkey
| Key combination to use for going back from KVM port to UI.
ConnectKey | connectkey
| Key to use to trigger switch to KVM port.
LocalUserAuthMode | authMode
| Authentication mode for local UI.
boolean | ignoreCCManagedMode
| Whether to allow local UI login under CC-SG management.

## Detailed Description

Local port settings.

Definition at line 41 of file LocalPort.idl.

## Member Data Documentation

## ◆ authMode

LocalUserAuthMode radm::LocalPort::Settings::authMode

Authentication mode for local UI.

Definition at line 46 of file LocalPort.idl.

## ◆ connectkey

ConnectKey radm::LocalPort::Settings::connectkey

Key to use to trigger switch to KVM port.

Definition at line 45 of file LocalPort.idl.

## ◆ enabled

boolean radm::LocalPort::Settings::enabled

Whether local port UI is enabled or not.

Definition at line 42 of file LocalPort.idl.

## ◆ hotkey

HotKey radm::LocalPort::Settings::hotkey

Key combination to use for going back from KVM port to UI.

Definition at line 44 of file LocalPort.idl.

## ◆ ignoreCCManagedMode

boolean radm::LocalPort::Settings::ignoreCCManagedMode

Whether to allow local UI login under CC-SG management.

Definition at line 47 of file LocalPort.idl.

## ◆ keyboardLayout

KeyboardLayout radm::LocalPort::Settings::keyboardLayout

Keyboard language to use.

Definition at line 43 of file LocalPort.idl.

The documentation for this struct was generated from the following file:

- LocalPort.idl