Legrand / Raritan Xerus™ JSON-RPC API for Remote Access Devices like KX4-101, KX3G2

Loading...
Searching...
No Matches
Public Attributes | List of all members
radm::KvmPort::CimPortSettings Struct Reference

Settings for CIM-based ports. More...

`import "KvmPort.idl";`

## Public Attributes
boolean | dosResolutionCompensation
| Whether to compensate for issues with 640x480 or 720x400 video resolutions.
boolean | offsetCompensation
| Whether to compensate for non-centered video output.
CimNamingMode | namingMode
| Name transfer behavior when connecting a CIM to this port.

## Detailed Description

Settings for CIM-based ports.

Definition at line 93 of file KvmPort.idl.

## Member Data Documentation

## ◆ dosResolutionCompensation

boolean radm::KvmPort::CimPortSettings::dosResolutionCompensation

Whether to compensate for issues with 640x480 or 720x400 video resolutions.

Definition at line 94 of file KvmPort.idl.

## ◆ namingMode

CimNamingMode radm::KvmPort::CimPortSettings::namingMode

Name transfer behavior when connecting a CIM to this port.

Definition at line 96 of file KvmPort.idl.

## ◆ offsetCompensation

boolean radm::KvmPort::CimPortSettings::offsetCompensation

Whether to compensate for non-centered video output.

Definition at line 95 of file KvmPort.idl.

The documentation for this struct was generated from the following file:

- KvmPort.idl